brlapi_driverspecific(3)            BrlAPI            brlapi_driverspecific(3)



NAME
       brlapi_driverspecific - Raw and Suspend Modes mechanism.


SYNOPSIS
   Functions
       int BRLAPI_STDCALL brlapi_enterRawMode (const char *driver)
       int BRLAPI_STDCALL brlapi__enterRawMode (brlapi_handle_t *handle, const
           char *driver)
       int BRLAPI_STDCALL brlapi_leaveRawMode (void)
       int BRLAPI_STDCALL brlapi__leaveRawMode (brlapi_handle_t *handle)
       ssize_t BRLAPI_STDCALL brlapi_sendRaw (const void *buffer, size_t size)
       ssize_t BRLAPI_STDCALL brlapi__sendRaw (brlapi_handle_t *handle, const
           void *buffer, size_t size)
       ssize_t BRLAPI_STDCALL brlapi_recvRaw (void *buffer, size_t size)
       ssize_t BRLAPI_STDCALL brlapi__recvRaw (brlapi_handle_t *handle, void
           *buffer, size_t size)
       int BRLAPI_STDCALL brlapi_suspendDriver (const char *driver)
       int BRLAPI_STDCALL brlapi__suspendDriver (brlapi_handle_t *handle,
           const char *driver)
       int BRLAPI_STDCALL brlapi_resumeDriver (void)
       int BRLAPI_STDCALL brlapi__resumeDriver (brlapi_handle_t *handle)

Detailed Description
       If the application wants to directly talk to the braille terminal, it
       should use Raw Mode. In this special mode, the driver gives the whole
       control of the terminal to it: brltty doesn't work any more.

       For this, it simply has to call brlapi_enterRawMode(), then
       brlapi_sendRaw() and brlapi_recvRaw(), and finally give control back
       thanks to brlapi_leaveRawMode().

       Special care of the terminal should be taken, since one might
       completely trash the terminal's data, or even lock it! The application
       should always check for terminal's type thanks to
       brlapi_getDriverName().

       The client can also make brltty close the driver by using
       brlapi_suspendDriver(), and resume it again with brlapi_resumeDriver().
       This should not be used if possible: raw mode should be sufficient for
       any use. If not, please ask for features :)

Function Documentation
   int BRLAPI_STDCALL brlapi__enterRawMode (brlapi_handle_t * handle, const
       char * driver)
   int BRLAPI_STDCALL brlapi__leaveRawMode (brlapi_handle_t * handle)
   ssize_t BRLAPI_STDCALL brlapi__recvRaw (brlapi_handle_t * handle, void *
       buffer, size_t size)
   int BRLAPI_STDCALL brlapi__resumeDriver (brlapi_handle_t * handle)
   ssize_t BRLAPI_STDCALL brlapi__sendRaw (brlapi_handle_t * handle, const
       void * buffer, size_t size)
   int BRLAPI_STDCALL brlapi__suspendDriver (brlapi_handle_t * handle, const
       char * driver)
   int BRLAPI_STDCALL brlapi_enterRawMode (const char * driver)
       Switch to Raw mode

       TODO: document which functions work in raw mode.

       Parameters
           driver Specifies the name of the driver for which the raw
           communication will be established.

       Returns
           0 on success, -1 on error

   int BRLAPI_STDCALL brlapi_leaveRawMode (void)
       Leave Raw mode

       Returns
           0 on success, -1 on error

   ssize_t BRLAPI_STDCALL brlapi_recvRaw (void * buffer, size_t size)
       Get Raw data

       Parameters
           buffer points on a buffer where the function will store the
           received data;
           size holds the buffer size.

       Returns
           its size, -1 on error, or on interruption by a signal or a
           parameter change notification, in which case brlapi_errno will be
           BRLAPI_ERROR_LIBCERR and errno will be EINTR.

   int BRLAPI_STDCALL brlapi_resumeDriver (void)
       Resume braille driver

       Returns
           -1 on error

   ssize_t BRLAPI_STDCALL brlapi_sendRaw (const void * buffer, size_t size)
       Send Raw data

       Parameters
           buffer points on the data;
           size holds the packet size.

       Returns
           size on success, -1 on error

   int BRLAPI_STDCALL brlapi_suspendDriver (const char * driver)
       Suspend braille driver

       Parameters
           driver Specifies the name of the driver which will be suspended.

       Returns
           -1 on error

Author
       Generated automatically by Doxygen for BrlAPI from the source code.



Version 0.8                     Tue Feb 17 2026       brlapi_driverspecific(3)
