brlapi_misc(3)                      BrlAPI                      brlapi_misc(3)



NAME
       brlapi_misc

SYNOPSIS
   Functions
       int BRLAPI_STDCALL brlapi_pause (int timeout_ms)
       int BRLAPI_STDCALL brlapi__pause (brlapi_handle_t *handle, int
           timeout_ms)
       int BRLAPI_STDCALL brlapi_sync (void)
       int BRLAPI_STDCALL brlapi__sync (brlapi_handle_t *handle)

Detailed Description
Function Documentation
   int BRLAPI_STDCALL brlapi__pause (brlapi_handle_t * handle, int timeout_ms)
   int BRLAPI_STDCALL brlapi__sync (brlapi_handle_t * handle)
   int BRLAPI_STDCALL brlapi_pause (int timeout_ms)
       Waits until an event is received from the BrlAPI server

       Parameters
           timeout_ms specifies an optional timeout which can be zero for
           polling, or -1 for infinite wait

       Returns
           0 on timeout, -1 on error, or on interruption by a signal or a
           parameter change notification, in which case brlapi_errno will be
           BRLAPI_ERROR_LIBCERR and errno will be EINTR.

   int BRLAPI_STDCALL brlapi_sync (void)
       Synchronize against any pending exception, and returns it. This allows
       to synchronously catch exception raised by brlapi_write calls. This
       works by temporarily replacing the current exception handler by its own
       handler.

       Returns
           0 if no exception was pending, -1 if an exception was caught.

Author
       Generated automatically by Doxygen for BrlAPI from the source code.



Version 0.8                     Mon Apr 6 2026                  brlapi_misc(3)
