brlapi_param_properties_t(3)        BrlAPI        brlapi_param_properties_t(3)



NAME
       brlapi_param_properties_t

SYNOPSIS
       #include <brlapi_param.h>

   Data Fields
       brlapi_param_type_t type
       uint16_t arraySize
       uint16_t isArray:1
       uint16_t canRead:1
       uint16_t canWrite:1
       uint16_t canWatch:1
       uint16_t abiPadding1:4
       uint16_t hasSubparam:1

Detailed Description
       Structure that describes the properties of a parameter

Field Documentation
   uint16_t brlapi_param_properties_t::abiPadding1
   uint16_t brlapi_param_properties_t::arraySize
       If .isArray is true, the number of elements in the parameter's value;
       if .isArray is false then the number of elements in the parameter's
       value is always exactly one

   uint16_t brlapi_param_properties_t::canRead
       True if the parameter is readable

   uint16_t brlapi_param_properties_t::canWatch
       True if the parameter can be watched

   uint16_t brlapi_param_properties_t::canWrite
       True if the parameter is writable

   uint16_t brlapi_param_properties_t::hasSubparam
       whether the Parameter uses the subparam argument

   uint16_t brlapi_param_properties_t::isArray
       True if the parameter's value contains several values; < False means
       always axactly one

   brlapi_param_type_t brlapi_param_properties_t::type
       Type of the parameter's value


Author
       Generated automatically by Doxygen for BrlAPI from the source code.



Version 0.8                     Mon Apr 6 2026    brlapi_param_properties_t(3)
