brlapi_paramValuePacket_t(3)        BrlAPI        brlapi_paramValuePacket_t(3)



NAME
       brlapi_paramValuePacket_t

SYNOPSIS
       #include <brlapi_protocol.h>

   Data Fields
       uint32_t flags
       brlapi_param_t param
       uint32_t subparam_hi
       uint32_t subparam_lo
       unsigned char data [BRLAPI_MAXPARAMSIZE]

Detailed Description
       Structure of Parameter value or update

Field Documentation
   unsigned char brlapi_paramValuePacket_t::data[BRLAPI_MAXPARAMSIZE]
       Which sub-parameter being transmitted, lo 32bits

   uint32_t brlapi_paramValuePacket_t::flags
   brlapi_param_t brlapi_paramValuePacket_t::param
       Flags to tell how value was gotten

   uint32_t brlapi_paramValuePacket_t::subparam_hi
       Which parameter being transmitted

   uint32_t brlapi_paramValuePacket_t::subparam_lo
       Which sub-parameter being transmitted, hi 32bits


Author
       Generated automatically by Doxygen for BrlAPI from the source code.



Version 0.8                     Mon Apr 6 2026    brlapi_paramValuePacket_t(3)
